{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Foglio1","Foglio2","Foglio3"],"not_rendered":{"images":1,"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Foglio1","index":0,"n_rows":85,"n_cols":6,"rows_kept":85,"merged":[[8,2,8,7]],"flags":["formulas_cached_only"]}
[]
[null,null,"metalrota s.r.l."]
[null,null,"Via Bulgaria,  46 - 41100 MODENA - ITALY"]
[null,null,"Tel. +39-059-315204 Fax +39-059-450439 "]
[null,null,"URL: www.metalrota.it"]
[null,null,"E-mail: info@metalrota.it"]
[]
[]
[null,null,"Electric Motors Request Form"]
[]
[]
[null,"Company Name"]
[]
[null,"Address"]
[]
[null,"Telephone N.",{"$nulls":3},"Fax N."]
[]
[null,"E-mail"]
[]
[null,"Contact Reference"]
[]
[]
[null,"Power (W)",{"$nulls":3},"Quantity per batch  "]
[]
[null,"Nominal speed (rpm)"]
[]
[null,"Nominal torque (Nm)",{"$nulls":3},"Peack torque (Nm)"]
[]
[null,"Rotation sense","R",null,null,"L"]
[null,"(looking to motor head flange)"]
[null,null,"L                      R  "]
[]
[]
[null,"Duty","Short Service",null,null,"tl="]
[]
[null,"tl= service time (min)","Shifts",null,null,"Service % ="]
[]
[null,"tr= resting time (min)","Cyclic Service",null,null,"tl=                        tr="]
[]
[]
[null,"Voltage  (12, 24, 48, 72, 80V)",{"$nulls":3},"Other"]
[]
[null,"DC Motor wounds","Series wound 2 terminals",null,null,"Series wound 4 terminals"]
[]
[null,null,"Compound wound",null,null,"Separately Excited"]
[]
[null,null,"Shunt wound",null,null,"PM"]
[]
[null,"AC Motor","Speed sensor",null,null,"Thermal sensor"]
[]
[null,"Motor diameter (mm)"]
[]
[null,"Environment and required IP"]
[]
[null,"Flange type","B5"]
[]
[null,null,"B14"]
[]
[null,null,"Other flange type"]
[]
[null,null,"customized on request"]
[]
[null,"Max motor length (mm)"]
[]
[null,"Max motor diameter (mm)"]
[]
[null,"e/m brake","Yes",null,null,"No"]
[]
[null,"Incremental Encoder","Pulses (ppr)2048-6000",null,null,"Voltage   TTL "]
[]
[null,"Connector type (8 pin M12, 12 pin EML, cable)"]
[]
[null,"Absolute Encoder (specify)"]
[]
[null,"Thermal protection","Yes",null,null,"No"]
[]
[null,"Tacho generator","Yes",null,null,"No"]
[]
[null,"Clamp or foot mounting","Yes",null,null,"No"]
[]
[null,"Contactor (start relay)","Yes",null,null,"No"]
[]
[null,"Forced fan","Yes",null,null,"No"]
[]
[null,"NOTES:"]

{"sheet":"Foglio2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Foglio3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}